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JS Air Curtains Standesse Air Curtain Specification 


1. The Standesse is a smart looking air curtain with fast-heat wire elements, designed for horizontal installation, with a self-supporting galvanised steel casing.

2. The Standesse casing is finished with a structural epoxy-polyester paint finish, offered in standard RAL 9016 (White), with other RAL classic colours available on request. 

3. [bookmark: _Hlk221712899]As standard, the fans are ‘AC’ type with double inlet centrifugal design, featuring low noise levels. They use an external rotor motor, offer three selectable speeds, and come equipped with built-in thermal protection. Two power options are available to accommodate various mounting heights and operating conditions.

4. EC (electronically commutated) fans with low energy requirements can be specially ordered, offering enhanced energy efficiency, lower operating costs, and sophisticated control options.

5. The Standesse unit shall measure 335mm high by 560mm deep and can be supplied in various lengths ranging from 1.0m to 2.5m in 0.5m increments.

6. The unit is designed for exposed, horizontal mounting above doors utilising M8 threaded drop rods. Optional brackets may be specially ordered for overhead or wall mounting, including, wall ‘rail’ and ceiling supports.

7. The air inlet grille is perforated, with a 2 in 1 face filter that acts as a suction grille and filter to prevent particles from entering the air curtain. This removes the need to have a separate internal filter. Only routine cleaning or vacuuming is needed in normal conditions. 

8. The unit can be specified with two regulated heating options: ‘E’ type (electric element heating with three stages), or ‘V’ type (LPHW water coil).

9. E’ type electric units shall operate on 400V/50Hz three-phase power and include power contactors, with three standard heating stages.

10. ‘V’ type water heated units shall offer on/off or proportional heating control, depending on optional valve type selected.

11. The Standesse is equipped with an ‘AirGenio Prime’ controller, featuring intuitive touch screen display, built-in temperature sensor, 7-day timer, volt free contact, and automatic control with manual override. The AirGenio application offers advanced settings and remote control functions.

12. The AirGenio Prime system supports master and slave operation, with one master unit capable of controlling up to 10 slave units. Each master unit shall be supplied with 20m of control cable.

13. Optional AirGenio Prime gateways shall be available for enhanced connectivity. BMS Gateway shall enable integration using Modbus TCP or BACnet protocols. Cloud Gateway shall allow Prime-controlled devices to be monitored, controlled and managed remotely through a web interface from any location.

14. The Standesse air curtain is produced to ISO 9001 standards, fully run tested for reliability, with traceable documentation for quality, is CE & UKCA certified and compliant with relevant regulations. BIM files can be provided upon request.


15. The system is to be supplied by					www:	Standesse Air Curtain
JS Air Curtains Limited 								
City Gates, 2-4 Southgate 
Chichester 								
West Sussex 							Tel:	+44 (0)333 038 4240
PO19 8DJ	 							e-mail:	sales@jsaircurtains.com
United Kingdom							Website:	www.jsaircurtains.com
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