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JS Air Curtains Venesse Air Curtain Specification 


1. The Venesse air curtain features a compact, slim design for vertical installation on either side of an entrance, with self-supporting galvanised steel casing.

2. The Venesse casing is finished with a structural epoxy-polyester paint finish, offered in RAL 9016 (White), with other RAL classic colours available on request. 

3. [bookmark: _Hlk221712899]The unit operates using AC type fans with double inlet centrifugal design, featuring low noise levels. They use an external rotor motor, offer three selectable speeds, and come equipped with built-in thermal protection. 

4. The Venesse unit shall measure 2,457mm high by 606mm wide and 300mm deep. 

5. The unit is suitable for vertical installation to the left or right of a doorway. For extra wide doorways, units can be placed either side of the entrance to create a stronger thermal barrier.

6. For servicing, periodic cleaning or vacuuming of the grille is needed in normal conditions.

7. The unit can be specified with various regulated heating options: ‘S’ type (low-energy air only, unheated or recirculating ambient air), ‘E’ type (electric element heating with three stages), or ‘V’ type (LPHW water coil).

8. E’ type electric units shall operate on 400V/50Hz three-phase power and include power contactors, with two standard heating stages.

9. ‘V’ type water heated units shall offer on/off or proportional heating control, depending on optional valve type selected.

10. The Venesse comes equipped with the AirGenio ‘Comfort’ or ‘Superior’ controller, featuring an advanced colour touch screen display, intuitive operation control, 3 fan speeds, volt free contact, and BMS connectivity options. 

11. The AirGenio Comfort and Superior systems support master and slave operation, with one master unit capable of controlling up to 10 slave units.

12. The Venesse air curtain is produced to ISO 9001 standards, fully run tested for reliability, with traceable documentation for quality, is CE & UKCA certified and compliant with relevant regulations. BIM files can be provided upon request.


13. The system is to be supplied by					www:	Venesse Air Curtain
JS Air Curtains Limited 								
City Gates, 2-4 Southgate 
Chichester 								
West Sussex 							Tel:	+44 (0)333 038 4240
PO19 8DJ	 							e-mail:	sales@jsaircurtains.com
United Kingdom							Website:	www.jsaircurtains.com
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